/** \file
 *
 *  This file contains special DoxyGen information for the generation of the main page and other special
 *  documentation pages. It is not a project source file.
 */
 
/** \mainpage Keyboard Host With HID Descriptor Parser Demo
 *  
 *  Keyboard host demonstration application. This gives a simple reference
 *  application for implementing a USB Keyboard host, for USB keyboards using
 *  the standard Keyboard HID profile. It uses a HID parser for the HID reports,
 *  allowing for correct operation across all USB keyboards. This demo supports
 *  keyboards with a single HID report.
 *  
 *  Pressed alpha-numeric, enter or space key is transmitted through the serial
 *  USART at serial settings 9600, 8, N, 1. On connection to a USB keyboard, the
 *  report items will be processed and printed as a formatted list through the
 *  USART before the keyboard is fully enumerated.
 *  
 *  Currently only single interface keyboards are supported.	
 *
 *  <table>
 *   <tr>
 *    <td><b>USB Mode:</b></td>
 *    <td>Host</td>
 *   </tr>
 *   <tr>
 *    <td><b>USB Class:</b></td>
 *    <td>Human Interface Device (HID)</td>
 *   </tr>
 *   <tr> 
 *    <td><b>USB Subclass:</b></td>
 *    <td>N/A</td>
 *   </tr>
 *   <tr>
 *    <td><b>Relevant Standards:</b></td>
 *    <td>USBIF HID Specification, USBIF HID Usage Tables</td>
 *   </tr>
 *   <tr>
 *    <td><b>Usable Speeds:</b></td>
 *    <td>Low Speed Mode, Full Speed Mode</td>
 *   </tr>
 *  </table>
 */