/** \file
 *
 *  This file contains special DoxyGen information for the generation of the main page and other special
 *  documentation pages. It is not a project source file.
 */
 
/** \mainpage CDC Class USB AVR Bootloader
 * 
 * This bootloader enumerates to the host as a CDC Class device (virtual serial port), allowing for AVR109
 * protocol compatible programming software to load firmware onto the AVR.	
 *  
 * Out of the box this bootloader builds for the USB1287, and will fit into 4KB of bootloader space. If
 * you wish to enlarge this space and/or change the AVR model, you will need to edit the BOOT_START and MCU
 * values in the accompanying makefile.
 *  
 * This bootloader is compatible with the open source application AVRDUDE, or Atmel's AVRPROG.
 *
 * <table>
 *  <tr>
 *   <td><b>USB Mode:</b></td>
 *   <td>Device</td>
 *  </tr>
 *  <tr>
 *   <td><b>USB Class:</b></td>
 *   <td>Communications Device Class (CDC)</td>
 *  </tr>
 *  <tr> 
 *   <td><b>USB Subclass:</b></td>
 *   <td>Abstract Control Model (ACM)</td>
 *  </tr>
 *  <tr>
 *   <td><b>Relevant Standards:</b></td>
 *   <td>USBIF CDC Class Standard</td>
 *  </tr>
 *  <tr>
 *   <td><b>Usable Speeds:</b></td>
 *   <td>Full Speed Mode</td>
 *  </tr>
 * </table>
 */
