/** \file
 *
 *  This file contains special DoxyGen information for the generation of the main page and other special
 *  documentation pages. It is not a project source file.
 */
 
/** \mainpage Mass Storage Host Demo
 *  
 *  Mass Storage host demonstration application. This gives a simple reference
 *  application for implementing a USB Mass Storage host, for USB storage devices
 *  using the standard Mass Storage USB profile.
 *  
 *  The first 512 bytes (boot sector) of an attached disk's memory will be dumped
 *  out of the serial port in HEX and ASCII form when it is attached to the AT90USB1287
 *  AVR. The device will then wait for HWB to be pressed, whereupon the entire ASCII contents
 *  of the disk will be dumped to the serial port.
 *
 *  <table>
 *   <tr>
 *    <td><b>USB Mode:</b></td>
 *    <td>Host</td>
 *   </tr>
 *   <tr>
 *    <td><b>USB Class:</b></td>
 *    <td>Mass Storage Device</td>
 *   </tr>
 *   <tr> 
 *    <td><b>USB Subclass:</b></td>
 *    <td>Bulk Only</td>
 *   </tr>
 *   <tr>
 *    <td><b>Relevant Standards:</b></td>
 *    <td>USBIF Mass Storage Standard</td>
 *    <td>USB Bulk-Only Transport Standard</td>
 *    <td>SCSI Primary Commands Specification</td>
 *    <td>SCSI Block Commands Specification</td>
 *   </tr>
 *   <tr>
 *    <td><b>Usable Speeds:</b></td>
 *    <td>Full Speed Mode</td>
 *   </tr>
 *  </table>
 */