/** \file
 *
 *  This file contains special DoxyGen information for the generation of the main page and other special
 *  documentation pages. It is not a project source file.
 */

/** \page Page_VIDPID VID and PID values
 *
 *  The LUFA library uses VID/PID combinations generously donated by Atmel. The following VID/PID combinations
 *  are used within the LUFA demos, and thus may be re-used by derivations of each demo. Free PID values may be
 *  used by future LUFA demo projects.
 *
 *  These VID/PID values should not be used in commercial designs under any circumstances. Private projects may
 *  use the following values freely, but must accept any collisions due to other LUFA derived private projects
 *  sharing identical values. It is suggested that private projects using interfaces compatible with existing
 *  demos share the save VID/PID value.
 *
 *  <table>
 *
 *   <tr>
 *    <td>
 *     <b>VID</b>
 *    </td>
 *    <td>
 *     <b>PID</b>
 *    </td>
 *    <td>
 *     <b>Usage</b>
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2040
 *    </td>
 *    <td>
 *     Test Application
 *    </td>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2041
 *    </td>
 *    <td>
 *     Mouse Demo Application (and derivatives)
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2042
 *    </td>
 *    <td>
 *     Keyboard Demo Application (and derivatives)
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2043
 *    </td>
 *    <td>
 *     Joystick Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2044
 *    </td>
 *    <td>
 *     CDC Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2045
 *    </td>
 *    <td>
 *     Mass Storage Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2046
 *    </td>
 *    <td>
 *     Audio Output Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2047
 *    </td>
 *    <td>
 *     Audio Input Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2048
 *    </td>
 *    <td>
 *     MIDI Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2049
 *    </td>
 *    <td>
 *     MagStripe Project
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204A
 *    </td>
 *    <td>
 *     CDC Bootloader
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204B
 *    </td>
 *    <td>
 *     USB to Serial Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204C
 *    </td>
 *    <td>
 *     RNDIS Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204D
 *    </td>
 *    <td>
 *     Keyboard and Mouse Combination Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204E
 *    </td>
 *    <td>
 *     Dual CDC Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204F
 *    </td>
 *    <td>
 *     AVRISP Programmer Project
 *    </td>
 *   </tr>
 *
 *  </table>
 */
